|  |  |  |  |
| --- | --- | --- | --- |
| **OOR Number**: |       | **Dealer:** |       |
| **Project Name:** |       | **Date:** |       |
|  |

[ ]  🡸 Check for **ALL** **Standard Default** selections

|  |  |
| --- | --- |
| **1.** | **Drawer Suspension** |
|  | [ ]  | Self-closing, self-centering, hold open feature. 100-pound drawer runs – **Standard Default**  |
|  | [ ]  | SEFA 8 150-pound full extension drawer slides – **Standard Default on file drawers**  |
|  |
| **2.** | **Hinges** |
|  | [ ]  | Stainless steel – **Standard Default** |
|  |
| **3.** | **Pull Locations** |
|  | Standard MAX/Lab polypropylene pull locations – horizontal on base cabinet doors and drawers |
|  | – **Standard Default**  |
|  |  | ***Wall, upper, and tall cases feature vertical pulls*** |
|  |
| **4.** | **Pull Types** |
|  | [ ]  | Semi-recessed polypropylene |
|  |  | [ ]  | Chameleon – **Standard Default** |
|  |  | [ ]  | Black |
|  |  | [ ]  | Gray |
|  |  | [ ]  | White |
|  |
| **5.** | **Door Catches** |
|  | [ ]  | Roller catch – **Standard Default**  |
|  |
| **6.** | **Lock Types** |
|  | Designated by cabinet suffix “**L**” |
|  | [ ]  | Master 5-disc – **Standard Default**Use when up to 225 primary key changes are required (master-keyed) |
|  | [ ]  | Master 5-pin |
|  |
| **7.** | **Glass** |
|  | Framed and/or unframed doors |
|  | [ ]  | Float glass – clear 6 mm – **Standard Default** |
|  | [ ]  | Safety glass – laminated 6 mm (framed)  |
|  | [ ]  | Safety glass – tempered 6 mm (framed) |
|  |
| **8.** | **Security Panel** |
|  | Between locked sections |
|  | [ ]  | Without security panel – **Standard Default** |
|  | [ ]  | With security panel |